Lab 12 – Series/Parallel Inductors

Names: ­­­­­­­­­­­­­­­­Nathaniel Paulus, Seth Wills

Date: 2017-12-07

The purpose of this lab is to:

Experiment with series circuits and parallel combinations of inductors.

The following inductors are needed (1 each of the following): 1mH, 2.2mH and 4.7mH

Measure and record the inductance of each inductor using the LCR meter. Connect the inductors as shown in Figure 1 and measure and record the total inductance, LT. Then connect the inductors as shown in Figure 2 and measure and record the total inductance, LT.

Equipment needed:

1 – LCR Meter



Figure 1

**Series Circuit**

1 – Elvis II

3 – Inductors

|  |  |  |  |
| --- | --- | --- | --- |
|  | Expected | Simulated | Measured |
| L1 = | 1mH | 1mH | 1.0194mH |
| L2 = | 2.2mH | 2.2mH | 2.1732mH |
| L3 = | 4.7mH | 4.7mH | 4.3352mH |
| LT = | 7.900mH | 7.90mH | 7.2047mH |

Expected = value you expect it to be

Simulated = using Multisim

Measured = using LCR Meter

|  |  |  |  |
| --- | --- | --- | --- |
|  | Expected | Simulated | Measured |
| L1 = | 1mH | 1mH | 1.0194mH |
| L2 = | 2.2mH | 2.2mH | 2.1732mH |
| L3 = | 4.7mH | 4.7mH | 4.3352mH |
| LT = | 599.768uH | 599.826uH | 561.09uH |

Expected = value you expect it to be

Simulated = using Multisim

Measured = using LCR Meter



Figure 2

**Parallel Circuit**

Observations: Inductance increases when put in series, and decreases when put in parallel.